*************************** START ****************************

START TIME: 202210061628

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xfae20850
mac h: 0xf412
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 14896 bytes (10242 compressed) at 0x00000000 in 0.1 seconds (effective 930.1 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (128 compressed) at 0x00008000 in 0.0 seconds (effective 4928.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 21899.1 kbit/s)...

Hash of data verified.
Wrote 552016 bytes (323454 compressed) at 0x00010000 in 4.8 seconds (effective 913.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 7 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202210061628

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xfae20850
mac h: 0xf412
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 14896 bytes (10242 compressed) at 0x00000000 in 0.1 seconds (effective 923.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (128 compressed) at 0x00008000 in 0.0 seconds (effective 4932.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 16428.3 kbit/s)...

Hash of data verified.
Wrote 552016 bytes (323454 compressed) at 0x00010000 in 4.8 seconds (effective 911.5 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 7 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202210061644

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xfae20850
mac h: 0xf412
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 14896 bytes (10242 compressed) at 0x00000000 in 0.1 seconds (effective 932.7 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (128 compressed) at 0x00008000 in 0.0 seconds (effective 4928.2 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 16425.3 kbit/s)...

Hash of data verified.
Wrote 552016 bytes (323454 compressed) at 0x00010000 in 4.8 seconds (effective 915.2 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 7 s

Download result: PASS

*************************** END ****************************



